#!/bin/sh /etc/rc.common
#
# Copyright (C) 2017 openwrt-ssr
# Copyright (C) 2017 yushi studio <ywb94@qq.com>
# Copyright (C) 2018 lean <coolsnowwolf@gmail.com>
#
# This is free software, licensed under the GNU General Public License v3.
# See /LICENSE for more information.
#

START=99
STOP=15

SERVICE_DAEMONIZE=1
NAME=vssr
EXTRA_COMMANDS=rules

#定义配置文件名称
CONFIG_FILE=/var/etc/${NAME}_t.json
CONFIG_UDP_FILE=/var/etc/${NAME}_u.json
CONFIG_SOCK5_FILE=/var/etc/${NAME}_s.json
CRON_FILE=/etc/crontabs/root

#定义可执行文件路径
VSSR_RULES_BIN=/usr/bin/vssr-rules

#初始化配置
server_count=0
redir_tcp=0
redir_udp=0
tunnel_enable=0
local_enable=0
kcp_enable_flag=0
kcp_flag=0
pdnsd_enable_flag=0
switch_enable=0
shunt_enable=0
switch_server=$1
MAXFD=32768
threads=1


#读取 uci 数据
uci_get_by_name() {
    local ret=$(uci get $NAME.$1.$2 2>/dev/null)
    echo ${ret:=$3}
}

uci_get_by_type() {
    local ret=$(uci get $NAME.@$1[0].$2 2>/dev/null)
    echo ${ret:=$3}
}

run_mode=$(uci_get_by_type global run_mode)
is_xray=$(uci_get_by_type global use_xray)

#查找可执行文件
find_bin() {
    case "$1" in
    ss) ret="ss-redir" ;;
    ss-local) ret="ss-local" ;;
    ssr) ret="ssr-redir" ;;
    ssr-local) ret="ssr-local" ;;
    ssr-server) ret="ssr-server" ;;
    v2ray | vless) ret="xray" ;;
    trojan) ret="trojan" ;;
    esac
    echo $(find /usr -perm /+x -type f -name $ret)
}

#添加定时执行脚本
add_cron() {
    sed -i '/vssr.log/d' $CRON_FILE && echo '0 1 * * * echo "" > /tmp/vssr.log' >>$CRON_FILE
    [ $(uci_get_by_type server_subscribe auto_update 0) -eq 1 ] && echo "0 $(uci_get_by_type server_subscribe auto_update_time) * * * /usr/bin/lua /usr/share/vssr/subscribe.lua" >>$CRON_FILE
    [ $(uci_get_by_type server_subscribe auto_update 0) -eq 1 ] && echo "0 $(uci_get_by_type server_subscribe auto_update_time) * * * /usr/bin/lua /usr/share/vssr/update.lua" >>$CRON_FILE
    crontab $CRON_FILE
}

#删除定时执行脚本
del_cron() {
    sed -i '/vssr/d' $CRON_FILE
    sed -i '/vssr.log/d' $CRON_FILE
    /etc/init.d/cron restart
}

#计算分流数量
count_shunt() {
    snum=0
    eval shunt_array1="youtube"
    eval shunt_array2="tw_video"
    eval shunt_array3="netflix"
    eval shunt_array4="disney"
    eval shunt_array5="prime"
    eval shunt_array6="tvb"
    eval shunt_array7="custom"
    for i in 1 2 3 4 5 6 7; do
        a=$(eval echo "\$shunt_array$i")
        local server_index=$(uci_get_by_type global ${a}_server)
        local server_type=$(uci_get_by_name $server_index type)
        if [ "$server_type" != "" ]; then
            snum=$(($snum + 1))
        fi
    done
    echo $snum
}


#创建配置文件
gen_config_file() {
    local hostip=$(uci_get_by_name $1 server)
    [ $2 = "0" -a $kcp_flag = "1" ] && hostip="127.0.0.1"

    if [ $2 = "0" ]; then
        re_type="tcp"
        config_file=$CONFIG_FILE
        server_obj=$GLOBAL_SERVER
    elif [ $2 = "1" ]; then
        re_type="udp"
        config_file=$CONFIG_UDP_FILE
        server_obj=$UDP_RELAY_SERVER
    fi
    [[ $(uci_get_by_name $1 fast_open 0) = "1" ]] && fastopen="true" || fastopen="false"

    local stype=$(uci_get_by_name $1 type)
    local port=$(uci_get_by_name $1 local_port)
    [[ "$stype" == "vless" ]] &&  stype="v2ray"

    if [ "$stype" == "trojan" ]; then
        if [ "$re_type" == "udp" ]; then
            re_type="client"
            port="10801"
        else
            re_type="nat"
        fi
    fi

    local mport=0
    if [ $3 = "1" ]; then
        stype="v2ray"
        mport=1090
        re_type="tcp"
    fi

    lua /usr/share/vssr/genconfig_${stype}.lua ${server_obj} ${re_type} ${port} ${hostip} ${mport} >${config_file}
    sed -i 's/\\//g' $config_file
}

#获取arg输出
get_arg_out() {
    case "$(uci_get_by_type access_control router_proxy 1)" in
    1) echo "-o" ;;
    2) echo "-O" ;;
    esac
}

#启动规则
start_rules() {
    local server=$(uci_get_by_name $GLOBAL_SERVER server)
    #resolve name
    if echo $server | grep -E "^[0-9]{1,3}\.[0-9]{1,3}\.[0-9]{1,3}\.[0-9]{1,3}$" >/dev/null; then
        server=${server}
    elif [ "$server" != "${server#*:[0-9a-fA-F]}" ]; then
        server=${server}
    else
        server=$(ping ${server} -s 1 -c 1 | grep PING | cut -d'(' -f 2 | cut -d')' -f1)
        if echo $server | grep -E "^[0-9]{1,3}\.[0-9]{1,3}\.[0-9]{1,3}\.[0-9]{1,3}$" >/dev/null; then
            echo $server >/etc/ssr_ip
        else
            server=$(cat /etc/ssr_ip)
        fi
    fi

    kcp_server=$server

    local kcp_enable=$(uci_get_by_name $GLOBAL_SERVER kcp_enable 0)
    if [ $kcp_enable = "1" ]; then
        kcp_flag=1
    fi

    local local_port=$(uci_get_by_name $GLOBAL_SERVER local_port)
    local lan_ac_ips=$(uci_get_by_type access_control lan_ac_ips)
    local lan_ac_mode=$(uci_get_by_type access_control lan_ac_mode)
    local router_proxy=$(uci_get_by_type access_control router_proxy)
    if [ "$GLOBAL_SERVER" == "$UDP_RELAY_SERVER" -a $kcp_flag == 0 ]; then
        ARG_UDP="-u"
    elif [ -n "$UDP_RELAY_SERVER" ]; then
        ARG_UDP="-U"
        local udp_server=$(uci_get_by_name $UDP_RELAY_SERVER server)
        if echo $udp_server | grep -E "^[0-9]{1,3}\.[0-9]{1,3}\.[0-9]{1,3}\.[0-9]{1,3}$" >/dev/null; then
            udp_server=${udp_server}
        elif [ "$udp_server" != "${udp_server#*:[0-9a-fA-F]}" ]; then
            udp_server=${udp_server}
        else
            udp_server=$(ping ${udp_server} -s 1 -c 1 | grep PING | cut -d'(' -f 2 | cut -d')' -f1)
            if echo $udp_server | grep -E "^[0-9]{1,3}\.[0-9]{1,3}\.[0-9]{1,3}\.[0-9]{1,3}$" >/dev/null; then
                echo $udp_server >/etc/ssr_ip
            else
                udp_server=$(cat /etc/ssr_ip)
            fi
        fi
        local udp_local_port=$(uci_get_by_name $UDP_RELAY_SERVER local_port)
    fi

    if [ -n "$lan_ac_ips" ]; then
        case "$lan_ac_mode" in
        w | W | b | B) local ac_ips="$lan_ac_mode$lan_ac_ips" ;;
        esac
    fi

    #deal	gfw firewall rule
    local gfwmode=""
    case "$run_mode" in
        gfw) gfwmode="-g" ;;
        router) gfwmode="-r" ;;
        oversea) gfwmode="-c" ;;
        all) gfwmode="-z" ;;
    esac

    local dports=$(uci_get_by_type global dports 1)
    if [ $dports = "1" ]; then
        proxyport=" "
    else
        proxyport="-m multiport --dports 22,53,587,465,995,993,143,80,443,9418"
    fi

    $VSSR_RULES_BIN \
    -s "$server" \
    -l "$local_port" \
    -S "$udp_server" \
    -L "$udp_local_port" \
    -a "$ac_ips" \
    -i "$(uci_get_by_type access_control wan_bp_list)" \
    -b "$(uci_get_by_type access_control wan_bp_ips)" \
    -w "$(uci_get_by_type access_control wan_fw_ips)" \
    -p "$(uci_get_by_type access_control lan_fp_ips)" \
    -G "$(uci_get_by_type access_control lan_gm_ips)" \
    -D "$proxyport" \
    $(get_arg_out) $gfwmode $ARG_UDP
    return $?
}

#启动PDNSD
start_pdnsd() {
    local usr_dns="$1"
    local usr_port="$2"

    local tcp_dns_list="208.67.222.222, 208.67.220.220"
    [ -z "$usr_dns" ] && usr_dns="8.8.8.8"
    [ -z "$usr_port" ] && usr_port="53"

    [ -d /var/etc ] || mkdir -p /var/etc

    if [ ! -d /var/pdnsd ]; then
        mkdir -p /var/pdnsd
        echo -ne "pd13\000\000\000\000" >/var/pdnsd/pdnsd.cache
        chown -R nobody:nogroup /var/pdnsd
    fi

    cat <<-EOF >/var/etc/pdnsd.conf
			global{
			perm_cache=1024;
			cache_dir="/var/pdnsd";
			pid_file="/var/run/pdnsd.pid";
			run_as="nobody";
			server_ip=127.0.0.1;
			server_port=5335;
			status_ctl=on;
			query_method=tcp_only;
			min_ttl=1h;
			max_ttl=1w;
			timeout=10;
			neg_domain_pol=on;
			proc_limit=2;
			procq_limit=8;
			par_queries=1;
			}
			server{
			label="ssr-usrdns";
			ip=$usr_dns;
			port=$usr_port;
			timeout=6;
			uptest=none;
			interval=10m;
			purge_cache=off;
			}
		EOF
    /usr/sbin/pdnsd -c /var/etc/pdnsd.conf -d
}


#开启分流
start_shunt() {
    eval shunt_type1="global"
    eval shunt_type2="youtube"
    eval shunt_type3="tw_video"
    eval shunt_type4="netflix"
    eval shunt_type5="disney"
    eval shunt_type6="prime"
    eval shunt_type7="tvb"
    eval shunt_type8="custom"
    eval shunt_port1=2080
    eval shunt_port2=2081
    eval shunt_port3=2082
    eval shunt_port4=2083
    eval shunt_port5=2084
    eval shunt_port6=2085
    eval shunt_port7=2086
    eval shunt_port8=2087
    for i in 1 2 3 4 5 6 7 8; do
        shunt_type=$(eval echo "\$shunt_type$i")
        shunt_port=$(eval echo "\$shunt_port$i")
        local server_index=$(uci_get_by_type global ${shunt_type}_server)
        local server_port=${shunt_port}
        local server_type=$(uci_get_by_name $server_index type)
        local server_ip=$(uci_get_by_name $server_index server)
        if [ "$server_type" = "vless" ]; then
            server_type="v2ray"
        fi
        [ "$server_type" = "trojan" ] && re_type="client" || re_type="tcp"
        if [ "$server_type" != "v2ray" -a "$server_type" != "" ]; then
            local config_file=/var/etc/${NAME}_${shunt_type}.json
            local bin=$(find_bin $server_type)
            lua /usr/share/vssr/genconfig_${server_type}.lua ${server_index} ${re_type} ${server_port} ${server_ip} >${config_file}
            sed -i 's/\\//g' $config_file
            case "$server_type" in
            ss | ssr)
                bin=$(find_bin "ss-local")
                [ "$server_type" == "ssr" ] && bin=$(find_bin "ssr-local")
                $bin -c $config_file $ARG_OTA -f /var/run/vssr-${shunt_type}.pid1 >/dev/null 2>&1
                ;;
            trojan)
                $bin --config $config_file >/dev/null 2>&1 &
                ;;
            esac
            echo "$(date "+%Y-%m-%d %H:%M:%S") ${shunt_type}: $server_type 分流服务已启动!" >>/tmp/vssr.log
        fi
    done
    return $?
}

start_redir() {
    case "$(uci_get_by_name $GLOBAL_SERVER auth_enable)" in
    1 | on | true | yes | enabled) ARG_OTA="-A" ;;
    *) ARG_OTA="" ;;
    esac

    #deal kcp
    local kcp_enable=$(uci_get_by_name $GLOBAL_SERVER kcp_enable 0)
    if [ $kcp_enable = "1" ]; then
        [ ! -f "/usr/bin/kcptun-client" ] && return 1

        local kcp_str=$(/usr/bin/kcptun-client -v | grep kcptun | wc -l)
        [ "0" = $kcp_str ] && return 1
        local kcp_port=$(uci_get_by_name $GLOBAL_SERVER kcp_port)
        local server_port=$(uci_get_by_name $GLOBAL_SERVER server_port)
        local password=$(uci_get_by_name $GLOBAL_SERVER kcp_password)
        local kcp_param=$(uci_get_by_name $GLOBAL_SERVER kcp_param)
        [ "$password" != "" ] && password="--key "${password}
        service_start /usr/bin/kcptun-client \
        -r $kcp_server:$kcp_port \
        -l :$server_port $password $kcp_param
        kcp_enable_flag=1
    fi

    gen_config_file $GLOBAL_SERVER 0 0
    local stype=$(uci_get_by_name $GLOBAL_SERVER type)
    sscmd=$(find_bin $stype)

    

    if [ "$(uci_get_by_type global threads 0)" = "0" ]; then
        threads=$(cat /proc/cpuinfo | grep 'processor' | wc -l)
    else
        threads=$(uci_get_by_type global threads)
    fi
    #转发TCP
    redir_tcp=1
    scount=$(count_shunt)
    if [ $scount == "0" ]; then
        local last_config_file=$CONFIG_FILE
        case "$stype" in
        ss | ssr)
            local pid_file="/var/run/ssr-retcp.pid"
            local name="Shadowsocks"
            [ "$type" == "ssr" ] && name="ShadowsocksR"
            for i in $(seq 1 $threads); do
                $sscmd -c $last_config_file $ARG_OTA -f /var/run/ssr-retcp_$i.pid >/dev/null 2>&1
            done
            echo "$(date "+%Y-%m-%d %H:%M:%S") $name $threads 线程 已启动!" >>/tmp/vssr.log
            ;;
        v2ray | vless)
            $sscmd -config $last_config_file >/dev/null 2>&1 &
            echo "$(date "+%Y-%m-%d %H:%M:%S") $($sscmd -version | head -1) 已启动!" >>/tmp/vssr.log
            ;;
        trojan)
            for i in $(seq 1 $threads); do
                $sscmd -c $last_config_file >/dev/null 2>&1 &
            done
            echo "$(date "+%Y-%m-%d %H:%M:%S") $($sscmd -V 2>&1 | head -1) $threads 线程 已启动!" >>/tmp/vssr.log
            ;;
        esac
    else
        if [ $stype != "vray" ]; then
            #开启 v2ray 路由服务
            gen_config_file $GLOBAL_SERVER 0 1
            sscmd=$(find_bin "v2ray")
            local last_config_file=$CONFIG_FILE
            $sscmd -config $last_config_file >/dev/null 2>&1 &
            echo "$(date "+%Y-%m-%d %H:%M:%S") $($sscmd -version | head -1) 已启动!" >>/tmp/vssr.log
        fi

    fi

    #转发UDP
    if [ -n "$UDP_RELAY_SERVER" ]; then
        redir_udp=1
        local utype=$(uci_get_by_name $UDP_RELAY_SERVER type)
        ucmd=$(find_bin $utype)
        gen_config_file $UDP_RELAY_SERVER 1 0
        last_config_file=$CONFIG_UDP_FILE
        case "$utype" in
        ss | ssr)
            case "$(uci_get_by_name $UDP_RELAY_SERVER auth_enable)" in
            1 | on | true | yes | enabled) ARG_OTA="-A" ;;
            *) ARG_OTA="" ;;
            esac
            local name="Shadowsocks"
            [ "$type" == "ssr" ] && name="ShadowsocksR"
            pid_file="/var/run/ssr-reudp.pid"
            $ucmd -c $last_config_file $ARG_OTA -U -f /var/run/ssr-reudp.pid >/dev/null 2>&1
            echo "$(date "+%Y-%m-%d %H:%M:%S") UDP TPROXY Relay: $name 已启动!" >>/tmp/vssr.log
            ;;
        v2ray | vless)
            $ucmd -config $last_config_file >/dev/null 2>&1 &
            echo "$(date "+%Y-%m-%d %H:%M:%S") UDP TPROXY Relay: $($sscmd -version | head -1) 已启动!" >>/tmp/vssr.log
            ;;
        trojan)
            $ucmd --config $last_config_file >/dev/null 2>&1 &
            ipt2socks -U -4 -b 0.0.0.0 -s 127.0.0.1 -p 10801 -l $(uci_get_by_name $UDP_RELAY_SERVER local_port) >/dev/null 2>&1 &
            echo "$(date "+%Y-%m-%d %H:%M:%S") UDP TPROXY Relay: Trojan 已启动!" >>/tmp/vssr.log
            ;;
        esac
    fi

    #deal with dns

    if [ "$(uci_get_by_type global pdnsd_enable)" = "1" ]; then
        local dnsstr="$(uci_get_by_type global tunnel_forward 8.8.4.4:53)"
        local dnsserver=$(echo "$dnsstr" | awk -F ':' '{print $1}')
        local dnsport=$(echo "$dnsstr" | awk -F ':' '{print $2}')
        if [ "$run_mode" = "gfw" ]; then
            ipset add gfwlist $dnsserver 2>/dev/null
        elif [ "$run_mode" = "oversea" ]; then
            ipset add oversea $dnsserver 2>/dev/null
        else
            ipset add ss_spec_wan_ac $dnsserver nomatch 2>/dev/null
        fi
        start_pdnsd $dnsserver $dnsport
        pdnsd_enable_flag=1
    fi

    if [ "$(uci_get_by_type global enable_switch)" = "1" ]; then
        if [ "$(uci_get_by_name $GLOBAL_SERVER switch_enable)" = "1" ]; then
            if [ -z "$switch_server" ]; then
                local switch_time=$(uci_get_by_type global switch_time)
                local switch_timeout=$(uci_get_by_type global switch_timeout)
                service_start /usr/bin/vssr-switch start $switch_time $switch_timeout
                switch_enable=1
            fi
        fi
    fi
    add_cron

    return $?
}

gen_service_file() {
    [[ $(uci_get_by_name $1 fast_open) = "1" ]] && fastopen="true" || fastopen="false"
    cat <<-EOF >$2
		{
		    "server": "0.0.0.0",
		    "server_port": $(uci_get_by_name $1 server_port),
		    "password": "$(uci_get_by_name $1 password)",
		    "timeout": $(uci_get_by_name $1 timeout 60),
		    "method": "$(uci_get_by_name $1 encrypt_method)",
		    "protocol": "$(uci_get_by_name $1 protocol)",
		    "protocol_param": "$(uci_get_by_name $1 protocol_param)",
		    "obfs": "$(uci_get_by_name $1 obfs)",
		    "obfs_param": "$(uci_get_by_name $1 obfs_param)",
		    "fast_open": $fastopen
		}
	EOF
}

start_service() {
    [ $(uci_get_by_name $1 enable) = "0" ] && return 1
    let server_count=server_count+1
    if [ $server_count = 1 ]; then
        if ! (iptables-save -t filter | grep SSR-SERVER-RULE >/dev/null); then
            iptables -N SSR-SERVER-RULE && \
            iptables -t filter -I INPUT -j SSR-SERVER-RULE
        fi
    fi

    gen_service_file $1 /var/etc/${NAME}_${server_count}.json
    /usr/bin/ssr-server -c /var/etc/${NAME}_${server_count}.json -u -f /var/run/ssr-server${server_count}.pid >/dev/null 2>&1
    iptables -t filter -A SSR-SERVER-RULE -p tcp --dport $(uci_get_by_name $1 server_port) -j ACCEPT
    iptables -t filter -A SSR-SERVER-RULE -p udp --dport $(uci_get_by_name $1 server_port) -j ACCEPT
    return 0
}

gen_serv_include() {
    FWI=$(uci get firewall.vssr.path 2>/dev/null)
    [ -n "$FWI" ] || return 0
    if [ ! -f $FWI ]; then
        echo '#!/bin/sh' >$FWI
    fi
    extract_rules() {
        echo "*filter"
        iptables-save -t filter | grep SSR-SERVER-RULE | sed -e "s/^-A INPUT/-I INPUT/"
        echo 'COMMIT'
    }
    cat <<-EOF >>$FWI
		iptables-save -c | grep -v "SSR-SERVER" | iptables-restore -c
		iptables-restore -n <<-EOT
		$(extract_rules)
		EOT
	EOF

}
start_server() {
    SERVER_ENABLE=$(uci_get_by_type server_global enable_server)
    [ "$SERVER_ENABLE" = 0 ] && return 0
    mkdir -p /var/run /var/etc

    config_load $NAME
    config_foreach start_service server_config
    gen_serv_include
    return 0
}

start_local() {
    local socks_server=$(uci_get_by_type socks5_proxy enable_server)
    local http_server=$(uci_get_by_type http_proxy enable_server)

    if [ "$socks_server" = "0" -a "$http_server" = "0" ]; then
        return 1
    fi
    mkdir -p /var/run /var/etc

    lua /usr/share/vssr/genconfig_v2ray_s.lua >$CONFIG_SOCK5_FILE
    sed -i 's/\\//g' $config_file
    socksbin=$(find_bin "v2ray")
    $socksbin -config $CONFIG_SOCK5_FILE >/dev/null 2>&1 &
    local_enable=1
}

rules() {
    [ "$GLOBAL_SERVER" = "nil" ] && return 1
    mkdir -p /var/run /var/etc
    UDP_RELAY_SERVER=$(uci_get_by_type global udp_relay_server)
    [ "$UDP_RELAY_SERVER" = "same" ] && UDP_RELAY_SERVER=$GLOBAL_SERVER
    if start_rules; then
        return 0
    else
        return 1
    fi
}

start() {
    if [ -z "$switch_server" ]; then
        GLOBAL_SERVER=$(uci_get_by_type global global_server)
    else
        GLOBAL_SERVER=$switch_server
        switch_enable=1
    fi
    if rules; then
        if start_redir; then
            if [ -f "/tmp/dnsmasq.ssr" ]; then
                rm -rf /tmp/dnsmasq.ssr
            fi
            if [ -f "/tmp/dnsmasq.oversea" ]; then
                rm -rf /tmp/dnsmasq.oversea
            fi
            mkdir -p /tmp/dnsmasq.d
            if ! [ "$run_mode" = "oversea" ]; then
                mkdir -p /tmp/dnsmasq.ssr
                cp -rf /etc/vssr/gfw_list.conf /tmp/dnsmasq.ssr/
                cp -rf /etc/vssr/gfw_base.conf /tmp/dnsmasq.ssr/
                cp -rf /etc/vssr/ad.conf /tmp/dnsmasq.ssr/
                cat >/tmp/dnsmasq.d/dnsmasq-ssr.conf <<EOF
conf-dir=/tmp/dnsmasq.ssr
EOF
            else
                mkdir -p /tmp/dnsmasq.oversea
                cp -rf /etc/vssr/oversea_list.conf /tmp/dnsmasq.oversea/
                cat >/tmp/dnsmasq.d/dnsmasq-ssr.conf <<EOF
conf-dir=/tmp/dnsmasq.oversea
EOF
            fi
            if [ $(uci_get_by_type global adblock) = 0 ]; then
                rm -f /tmp/dnsmasq.ssr/ad.conf
            fi
            /usr/share/vssr/gfw2ipset.sh
        else
            /usr/bin/ssr-rules -f
        fi
    fi
    /etc/init.d/dnsmasq restart >/dev/null 2>&1
    start_server
    start_local
    scount=$(count_shunt)
    if [ $scount != "0" ]; then
        start_shunt
    fi
    if [ $(uci_get_by_type global monitor_enable) = 1 ]; then
        let total_count=server_count+redir_tcp+redir_udp+tunnel_enable+kcp_enable_flag+local_enable+pdnsd_enable_flag+switch_enable
        if [ $total_count -gt 0 ]; then
            #param:server(count) redir_tcp(0:no,1:yes)  redir_udp tunnel kcp local gfw
            service_start /usr/bin/vssr-monitor $server_count $redir_tcp $redir_udp $tunnel_enable $kcp_enable_flag $local_enable $pdnsd_enable_flag $switch_enable
        fi
    fi

    ENABLE_SERVER=$(uci_get_by_type global global_server)
    [ "$ENABLE_SERVER" = "nil" ] && return 1
}

boot() {
    (/usr/share/vssr/chinaipset.sh && sleep 5 && start >/dev/null 2>&1) &
}

stop() {
    echo "stop"
    /usr/bin/vssr-rules -f
    srulecount=$(iptables -L | grep SSR-SERVER-RULE | wc -l)
    if [ $srulecount -gt 0 ]; then
        iptables -F SSR-SERVER-RULE
        iptables -t filter -D INPUT -j SSR-SERVER-RULE
        iptables -X SSR-SERVER-RULE 2>/dev/null
    fi
    if [ -z "$switch_server" ]; then
        kill -9 $(busybox ps -w | grep vssr-switch | grep -v grep | awk '{print $1}') >/dev/null 2>&1
    fi
    if [ $(uci_get_by_type global monitor_enable) = 1 ]; then
        kill -9 $(busybox ps -w | grep vssr-monitor | grep -v grep | awk '{print $1}') >/dev/null 2>&1
    fi
    killall -q -9 ss-redir ss-local obfs-local ssr-redir ssr-local ssr-server xray-plugin xray trojan microsocks ipt2socks dns2socks pdnsd

    if [ -f "/tmp/dnsmasq.d/dnsmasq-ssr.conf" ]; then
        rm -rf /tmp/dnsmasq.d/dnsmasq-ssr.conf /tmp/dnsmasq.ssr /tmp/dnsmasq.oversea
        /etc/init.d/dnsmasq restart >/dev/null 2>&1
    fi
    del_cron
}
